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Product Parameters
[bookmark: _GoBack]GTRACKER-308 is a highly modular positioning product,Based on 4G communication network and GPS global satellite positioning system. Its Internet platform locates and monitors remote targets, and at the same time has functions such as ACC detection, mileage statistics, oil disconnection and power failure, and notifies the owner of the vehicle condition information through SMS and platform.This product supports various protocols such as JT808




Product advantages
· Intelligent positioning
· Remote control
· Motion alarm
· Fatigue driving
· Remote flameout
· Remote upgrade
· Trace play back
· Electronic fence
· Mileage statistics
· Power-off alarm
· Speed Alarm
· ACC detection







Parameters
	Item
	parameters

	Name
	4G Mini GPS Tracker

	Network
	4G/GSM/GPRS

	Network band
	FDD-LTE（B1/B3）/TDD-LTE(B38/B39/B40/B41)
850/900/1800/1900Mhz

	Standby power standby
	180mA/4.2V(optional)

	Power power independent working time
	About 0.5 hours

	Power waste
	< 40mA/12V

	Input power
	DC 9V~100V/1.5A

	Standby power standby
	180mA/4.2V(optional)

	GSM/GPRS modules
	CAT1

	GPS sensitivity
	-159dBm

	GPS accuracy
	5-10 meters

	Tracking sensitivity
	-165dBm

	The startup time for the first time
	cold start time:   45-120s
warm start time:   35s
hot start time:  1s

	Size
	75mm x 35mm x 15mm

	Weight
	50g

	Storage temperature
	-40°C to +85°C

	Operating temperature
	-30°C to +75°C

	Relative Humidity
	5%--95% non-condensing
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