LED Panel Specification
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Function
The status of MDVR can be viewed through the LED panel indicator light, and remote control signals can be received to remotely control MDVR. It is suitable for use in locations where MDVR installation is concealed and inconvenient for viewing status and control; The device also supports one click alarm function, and pressing the red ALM button on the panel can initiate an alarm to the platform.




Product Features
· Equipped with LED panel display
· One click alarm button
· Optional IR function












Key Function
	Item
	Instruction

	Indicator
	PWR
	Power Indicator

	
	NET
	Network indicator

	
	GPS
	Satellite positioning indicator

	
	HDD
	Hard Disk Indicator

	
	VLS
	Radar indicator

	
	HOT
	Heating indicator

	
	AP
	AP indicator

	
	SD
	SD card indicator

	Induction 
	IR
	Proximity sensor

	Key
	ALM
	Alarm button






Interface definition
[image: 6e7f64c3-10ac-4f75-bf56-a3242d22ca7e]
Definition of Equipment Tail Line Interface
1. Optional connector, first connect the device to the connector, and then connect the connector to MDVR's RS232 (recommended).
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2. Cut the wires yourself and connect to the RS232 interface of MDVR according to the device's tail line interface definition.
3. MDVR requires a 12V power supply for the device, with the TX of MDVR connected to the RX of the device and the RX connected to the TX of the device;
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4. In the "Serial Port Function" menu of MDVR, you need to change the RS232 serial port function to LED panel with a baud rate of 9600. After making the changes, save and restart MDVR to use it normally.
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