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Functions＆features
· Support multiple serial port expansion, can dock more sensors, peripherals, expansion function is stronger.
· Support 4ch RS232 interface, each interface can be set up and work independently.
· Support 1ch RS485 interface.
· Support 4ch switch alarm input, 2ch analog alarm input, 1ch alarm output; 
· Support 1ch PWM interface, input and output can be configured.



Technical Parameters
	Project
	Performance index

	Input interface
	power
	5V-12V

	
	GND
	1piece

	
	TXD(RS232)
	1 piece

	
	RXD(RS232)
	1 piece

	Indicator light
	power led
	The indicator light comes on when the power is on，When there is data interaction, the lights flicker

	Output interface
	RS232
	4 piece，independent work

	
	RS485
	1 piece

	
	I/O Alarm input
	4 piece

	
	Analog quantity alarm input
	2 piece

	
	Alarm output
	1 piece

	
	PWM
	1 piece，configurable

	
	power output
	5V@1A




Installation matters
· Input interface definition
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	PIN 
	Color
	Definition

	1
	red
	12V/5V

	2
	brown
	RXD

	3
	purple
	TXD

	4
	black
	GND





· Output interface definition
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	PIN
	color
	definition
	PIN
	color
	definition

	1
	brown
	RX2
	2
	brown
	RX1

	3
	purple
	TX2
	4
	purple
	TX1

	5
	brown
	RX4
	6
	brown
	RX3

	7
	purple
	TX4
	8
	purple
	TX3

	9
	white
	ALM_IN2
	10
	white
	ALM_IN1

	11
	white
	ALM_IN4
	12
	white
	ALM_IN3

	13
	gray
	ALM_OUT
	14
	white
	ADC_IN1

	15
	yellow
	485B
	16
	white
	ADC_IN2

	17
	orange
	485A
	18
	blue
	PWM

	19
	black
	GND
	20
	pink
	5V
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