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Parameters
	NO.
	Item
	Description

	Pixel tube
	Dot pitch
	7.62*6mm

	
	Pixel tube chip
	Taiwan Opto Lei

	
	Luminous point color
	1 yellow/red（9mil）

	
	Density
	27800点

	
	Base color
	Red/Yellow

	led
	Center wavelength
	Brightness
	led

	Pure Red R
	625
	1800mcd
	Pure Red R

	Cell board[image: P6单元板单黄]
	Module size
	768x122mm

	
	Number of rows and columns of unit board
	Wide 128 point× Hight 16 point

	
	Resolution
	27800/ m²

	
	Column driver IC
	74HC5026

	
	Row driver IC
	74HC4953

	
	Main control chip
	74HC245

	
	Relative temperature
	-40~+80℃

	
	Operating Voltage
	9-36V  50HZ

	
	Average power consumption
	25W

	Main technical parameters
	Drive way
	1/8

	
	Refresh rate
	≧100HZ

	
	Gray scale
	No

	
	Color
	Yellow/Red

	
	Video input/output method
	3G wireless network transmission

	
	Service life
	≧80000h

	Product Size
	frame size
	830*195*230mm

	
	[bookmark: _GoBack]display size
	Front：170*120mm
Rear：765*125mm
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