Taxi meter
Model：MX-Ha-01
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Product Introduction
The unique operation management function of this product effectively utilizes the intelligent advantages of the meter and hardware resources such as IC card readers and writers, combined with the designed taxi operation management software. It can transmit management information to the meter, collect and process operation information, and implement operation management, supervision, inspection, etc. This system can make the management of the taxi industry more scientific, efficient, and standardized.

· LCD display function
· Printing function
· Voice function
· Normal operation function at low temperature
· Operational pricing function
· Clock calibration function
· Data collection function



Product parameters
	Item
	Description

	Calculation error
	± 0.5%

	Timing error
	± 0.2%

	Switching speed error
	± 0.5km/h

	Permanent clock error
	± 5s/d

	Working voltage
	DC +9V～16V

	Working current
	≤ 150mA (excluding empty car light on)

	Current during printing
	 Needle printer ≤ 500mA Thermal printer ≤ 1500mA

	Working conditions
	 Temperature range of -20 ℃ to+70 ℃

	Humidity 
	≤ 90% RH

	Storage conditions
	Temperature -40 ℃ to+80 ℃

	Humidity 
	≤ 90% RH
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