TTS Voice Broadcast Specification
Model: MX-TTS-01-01
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	Parameters

	Function
	Support Chinese and English and mixed reading

	Composite text size
	Maximum 4K bytes supported

	Property
	volume、speed adjustable

	Interface
	RS232 interface

	Baud rate
	4800

	Operating temperature
	-20-70°C

	Power input
	DC 5V/0.05A

	Power protection
	Support Anti-reverse protection function 

	Consumption
	0.25W

	Function
	Support Chinese and English and mixed reading

	Size
	91*76.6*25.2mm
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