Product Model: MX-AHDH-113A-AXP-005, 2.8mm
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Features:
◎ Exquisite design, exquisite workmanship, precise circuit and rigorous structure, reflecting the highest technology;
◎Specialized strong adhesive design, easy to install;
◎Rotatable lens allows you to adjust the shooting angle;
◎Meet the needs of most commercial vehicles;
◎Image: positive image/mirror image;
◎Appearance color: black;
◎Specialized aviation interface design;
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Parameters and specifications:
	Plan
	FH8333+IMX662

	Image sensor
	1/2.8″ SONY AHD

	Resolution
	1080P

	Signal system
	PAL system

	Pixel
	1920（H) x 1080(V)

	lens
	2.8mm lens

	Camera angle
	100°

	Minimum illumination
	0.01Lux

	Backlight compensation
	automatic

	Shutter speed
	Automatic: 1/50~1/100,000 (seconds)

	White Balance
	Auto tracking white balance

	Wide dynamic range
	Greater than 120DB

	Signal-to-noise ratio
	Greater than 50db

	Video Output
	1.0Vp-p,75Ω

	power supply
	DC12V±10%

	Power consumption
	≤3W

	Operating temperature
	-20℃ ~ +70℃

	Infrared wavelength
	/

	Number of infrared lights
	/

	Infrared light irradiation distance
	/

	Infrared light illumination
	/

	Interface
	M12 aircraft carrier head (with O-ring)

	Dimensions
	72mm*58mm*78mm





Dimensions:
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