Product Model: MX-AHDH-115B-NNP-005, 2.1mm
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Features:
◎Exquisite design, fine workmanship, precise circuitry and rigorous structure, reflecting the highest level of technology;
◎Special strong adhesive design for easy installation;
◎The rotatable lens allows for adjustment of the shooting angle;
◎ Meets the needs of most commercial vehicles;
◎Image: Orthogonal/Mirror Image;
◎Appearance color: Black;




















Specifications:
	Plan
	8536H+2053

	Image sensor
	1/2.9″ CMOS AHD

	Image resolution
	1080P

	Signal system
	PAL

	Pixels
	1920 (H) x 1080 (V)

	lens
	2.1mm

	Maximum angle
	130°

	Minimum Illumination
	0Lux

	Backlight compensation
	built-in

	Shutter speed
	automatic

	White alance
	Automatic white balance tracking

	Wide dynamic range
	none

	Signal-to-noise ratio
	Greater than 50dB (AGC OFF)

	Video output
	1.0Vp-p, 75Ω

	Audio
	Optional

	Power supply
	DC12V±10%

	Power consumption
	Infrared light on/off ≤3W

	Operating temperature
	-20℃ ~ +70℃

	Infrared wavelength
	850

	Number of infrared lights
	5

	Infrared light illumination distance
	0-3 meters

	Infrared light illuminance
	0LUX

	Interface
	BMW Connector
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