Product model: MX-AHDH-260A-NXP-005H (Optional fisheye version)
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Product features:
· Exquisite design, exquisite workmanship, precise circuits and rigorous structure, reflecting the highest technology;
· Wide angle adjustable bracket, which can adjust the angle freely during the installation and fixation process;
· Equipped with a small sunshade protective cover;
· Waterproof sealed aluminum cover with waterproof effect;
· Integrated structure, shockproof and anti loosening design;
· Suitable for monitoring in various vehicle environments;
· Image: Ortho/Mirror.
· Appearance color: black;
· Special aviation interface design















Specification parameters:
	Model
	MX-AHDH-260A-NXP-005H

	Programme
	8550+2093（fisheye 8536H+2053）

	Image sensor
	1/2.9″ CMOS AHD 

	Resolution
	1080P

	Signal system
	PAL/NTSC

	Pixel
	1920（H) x 1080(V)

	Horizontal angle of view
	130°/160°/180°

	Minimum illumination
	0.01Lux

	Backlight compensation
	built-in

	White balance
	Automatic tracking of white balance

	Signal-to-noise ratio
	＞45db (AGC OFF)

	Video output
	1.0Vp-p,75Ω

	Source
	DC12V±10%

	Power consumption
	≤2W

	Working temperature
	-20℃ ~ +70℃

	Interface
	Professional aviation interface

	Appearance dimensions
	56.75mm*52.7mm*37.5mm
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