Product Model: MX-AHDM-267A-NNP-005H
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Features:
1. 1/ 2.9 " CMOS
2. Resolution: 1280*720L
3. Minimum illuminance: 0.01 Lux
4. Automatic electronic shutter, automatic exposure, automatic white balance
5. Supports 2.1 mm field of view lenses
6. Night vision: Infrared night vision
7. Waterproof, suitable for outdoor installation






















Specifications:
	Product Model
	MX-AHDM-267A-NNP-005H

	Imaging devices
	1/ 2.9 " CMOS

	resolution
	720P

	Standard
	P-system/25 frames

	Minimum Illumination
	0.01 lux

	Synchronization System
	Internal synchronization

	Scanning System
	line scan

	Signal-to-noise ratio
	≥50dB

	Electronic shutter
	1/25 to 1/25,000 of a second (automatic)

	Filter type
	Color box black and white switching

	White Balance
	Automatic white balance tracking

	Automatic gain
	support

	3D noise reduction
	support

	Backlight compensation
	support

	angle
	Field of view: Diagonal: 140 ° , Horizontal: 120 ° , Vertical: 68 °

	Image mode
	Colored bricks black and white

	Video output
	1.0Vp-p composite video output, 75 ohms, 4-pin aviation cable

	power supply
	DC12V -24V

	Power consumption
	Maximum 300mA/DC12V±5%

	Operating temperature
	-30°C ~ 75°C

	Operating humidity
	Humidity less than 95% (no condensation)

	Waterproof rating
	IP68

	Installation method
	bracket installation

	audio
	No audio




Size specifications :
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Wiring definition:
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