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Product feature
1.Exquisite design, exquisite workmanship, precise lines and rigorous structure, reflecting the highest technology; 
2.Integrated structure, shockproof, dust-proof, anti-fog design; 
3.Suitable for all kinds of vehicles；
4.Image: positive/mirror image；
5.Color: white;
6.Dedicated aviation interface design；

















Specification
	Model
	MX-AHDL-610A-NNP-005H

	Image Sensor + DSP
	1/2.7″ CMOS AHD

	Picture Pixels
	1920(H)*1080(V)

	Video Frame Rate
	PAL: 1080p@25fps, NTSC: 1080p@30fps

	Video Output
	AHD

	Transmission Distance
	More than 500m via 75-3 coaxial cable

	Minimum Illumination
	Day: 0.01Lux, 0Lux (IR ON)

	Lens
	2.8mm

	Horizontal angle of view
	Optional 90°/100°/105°

	Sync System
	Internal Synchronization

	Electronic Shutter
	PAL: 1/25 -1/50,000 Sec, NTSC: 1/30 -1/60,000 Sec

	S/N Ratio
	More than 50dB

	Day and Night
	Auto (ICR) / Color / B/W

	Infrared LED
	12mil*Φ5*12pcs LEDs 

	IR Distance
	10-15m

	OSD Menu
	Support

	UTC
	Support

	OSD/UTC Language
	EN, CN, DE, FRA, IT, ES, PL, RU, PT, NL, TR

	D-WDR
	Support

	Noise Reduction
	3D NR

	White Balance
	Auto / Manual

	Gain Control
	Auto

	Operation Temperature
	-20°C~+70°C / Less than 95%RH (No condensation)

	Power Supply
	DC12V+/-20%

	Dimension
	Φ120*62mm

	Housing
	Ivory color metal case
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