Model: MX-AHDH-701A-NNP-005H
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Features:
◎Low power consumption, easy heat dissipation; good color reproduction, clear picture quality;
◎Exquisite, beautiful and fashionable appearance;
◎Fashionable appearance; high strength, highly resistant to impact damage;
◎ Using 9 imported high-power LED lights, shooting distance 10 m;
◎Infrared automatically turns on when the light is lower than 10Lux;
◎Adopt imported lens to prevent water vapor from affecting the image;
◎Appearance color: black ;
◎ Waterproof grade: IP67 ;
◎Specialized aviation interface design .


















Specifications:
	Model
	MX-AHDH-701A-NNP-005H

	Image Sensor
	1/4″ CMOS AHD

	Resolution
	1080P/720P

	Signal system
	PAL / NTSC​

	Pixel
	1920 ( H) x 1080(V)

	Lenses
	2.8mm/3.6mm 

	Horizontal angle of view
	100°/80°

	Minimum illumination
	0.001 ( Lux ) (Infrared on)

	Backlight compensation
	built-in

	Shutter speed
	1/50~1/10000 seconds ( P ) 1/60-1/10000 seconds ( N )

	White Balance
	automatic

	Signal-to-Noise Ratio
	Greater than 50db (AGC OFF)

	Video Output
	AHD , amplitude 1Vp-p, 75Ω

	Power supply
	[bookmark: _GoBack]Rated DC12V±10%

	Power consumption
	Infrared light on Infrared light off ≤ 3W

	Operating temperature
	-20 ℃ ~ +70℃

	Infrared wavelength
	850nm

	Number of infrared lights
	Φ 5 12LED lamp

	Infrared light irradiation distance
	5M

	Infrared light illumination
	＞3Lux

	Jack
	M12 aircraft carrier head (with O -ring)

	Dimensions
	90mm*77.5mm*62mm
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