Model：MX-AHDH-705A-NNP-005H,2.8mm
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Product features:
· Exquisite design, exquisite workmanship, precise circuits and rigorous structure, reflecting the highest technology;
· Wide viewing angle adjustable bracket, which can adjust the angle freely during installation and fixation;
· Using Φ 5 11LED lights with an infrared distance of 10 meters;
· Specialized for monitoring on both sides of professional vehicles;
· Waterproof sealed mechanism, can be used outdoors;
· Integrated structure, shockproof and anti loosening design;
· Suitable for monitoring in various vehicle environments;
· Image: positive/mirror image.
· Appearance color: black;
· Specialized aviation interface design





Specification parameters：
	Image sensor
	1/2.9″ CMOS AHD    
	　

	Resolution
	720P
	1080P

	Signal system
	PAL/NTSC
	PAL/NTSC

	Pixel
	1280（H) x 720(V)
	1920（H) x 1080(V)

	Lens
	2.8mm /2.7mm
	2.8mm/2.7mm 

	Horizontal angle of view
	[bookmark: _GoBack]100°/130°
	100°/130°

	Minimum illumination
	0Lux
	0Lux

	Backlight compensation
	built-in
	built-in

	shutter speed
	1/53~1/100,000（S）
	1/53~1/100,000（S）

	white balance
	Automatically track white balance
	Automatically track white balance

	Signal to noise ratio
	>38db (AGC OFF)
	>38db (AGC OFF)

	Video output
	1.0Vp-p,75Ω
	1.0Vp-p,75Ω

	Power Supply
	DC12V±10%
	DC12V±10%

	Power consumption
	≤3W
	≤3W

	working temperature 
	-20℃ ~ +70℃
	-20℃ ~ +70℃

	Infrared wavelength
	850nm
	850nm

	IR LED Quantity 
	Φ5 11LED灯
	Φ5 11LED灯

	IR View Distance 
	10M
	10M

	Illuminance when the infrared light is turned on
	＞3Lux
	＞3Lux

	Jack
	VIDEO OUT (Professional aviation interface )
	VIDEO OUT (Professional aviation interface )

	Appearance size
	94.68mm*71.58mm*41.5mm
	94.68mm*71.58mm*41.5mm
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