Model: MX-AHDH-803-NNP-WIFI-H , 2.8mm
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Features:
1. Low power consumption and easy heat dissipation;
2. Wide viewing angle, adjustable stand,
3. Provide indoor and outdoor sun protection;
4. Waterproof grade, IP6 6 ;
5. Integrated structure, shockproof and anti-loosening design;
6. Applicable to various vehicle monitoring environments
7. Color: Black;
8. Suitable aviation connector design;
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	Model
	MX-AHDH-803-NNP-WIFI-H

	Wireless Camera

	Image Sensor
	1/2.9 inch CMOS

	Image resolution
	2MP

	Image pixels
	1920(horizontal)*1080(vertical)

	Video frame rate
	1080p@25fps or 30fps

	Minimum illumination
	Color: 0.01Lux, Black and White: 0.001Lux, 0Lux (infrared on)

	lens
	2.8mm 2MP IR plate lens (90°)

	Horizontal angle of view
	100°

	day and night
	Automatic (ICR) / Color / Black and White

	Infrared LED
	16 LED arrays

	Infrared distance
	10-15 meters

	Wide dynamic range
	Wide dynamic range

	Wireless
	Built-in 2.4GHz wireless signal receiver

	Operating temperature
	-20 ⁰ C-70 ⁰ C

	power supply
	DC 12V±20%

	shell
	IP66 rated black metal housing

	2.4G HD wireless waterproof receiver

	power supply
	DC12V-24V

	Emission current
	300 mAh

	Video Output
	720P (HD)

	Operating frequency
	2400-2483.5MHz

	Transmission distance
	500m open space

	Startup time
	3 seconds

	Transmission power
	12Mbps

	Pair
	automatic

	Sound
	No

	Water proof
	IP66

	Delay time
	9-120 ms

	Operating temperature
	-20 ～ 70 ℃ RH95% or less

	Storage temperature
	-30 ～ 80 ℃ RH95% or less

	Shell
	Black plastic housing

	Aspect
	80(length)*40(width)*18(thickness)mm

	Red light on/off
	Power on/off

	Flashing red light
	Pairing

	Green light on
	Connection successful

	Green light off
	Signal loss
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