Product Model: MX-AHDH-806A-NNP-005H
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Features:
[bookmark: _GoBack]◎Exquisite design, fine workmanship, precise circuitry and rigorous structure, reflecting the highest level of technology;
◎Integrated structure with shock-resistant and anti-loosening design;
◎Suitable for monitoring in various vehicle-mounted environments;
◎Appearance color: Black;
◎Dedicated aviation interface design


Specifications:

	Imaging devices
	1/ 2.9 CMOS

	Standard
	PAL

	Resolution
	1080P

	Pixels
	1 920 (H) * 1080 (V)

	Shutter speed
	  Automatic: 1/50 - 1/100,000 (s)

	Minimum Illumination
	0.01 Lux

	Video format
	AHD

	Wide dynamic range
	none

	aperture
	F2.2

	Signal-to-noise ratio
	Greater than 50 dB

	White Balance
	AUTO

	Backlight compensation
	automatic

	lens
	2.8 mm/ 3.6mm

	Horizontal angle of the lens
	100 ° / 85 °

	audio
	none

	Protection level
	IP68

	power
	≤3W

	Voltage
	DC 12V±10%

	Operating temperature
	-20°C to 70°C

	Storage temperature
	-30°C to 80°C
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