Model：MX-AHDH-813-ANP-015
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Product features：
· Exquisite design, exquisite workmanship, precise circuits and rigorous structure, reflecting the highest technology;
· Wide angle adjustable lens, which can adjust the angle freely during the installation and fixation process;
· Integrated structure, shockproof and anti loosening design;
· Suitable for monitoring in various vehicle environments;
· Image: positive/mirror image;
· Appearance color: black;
· Special aviation interface design with silicone sleeve and silicone ring.













Specifications:
	Model
	MX-AHDH-813-ANP-015

	Image sensor
	1/2.9″ CMOS AHD

	Signal system
	PAL

	Pixel
	1920(H) x 1080(V)

	Lens
	3.6mm/2.1MM

	Horizontal angle of view
	85°/130°

	Minimum illumination
	0Lux

	Backlight compensation
	Built-in

	Shutter speed
	1/53~1/100,000（Sec）

	White balance
	Auto Tracing White Balance

	Signal-to-noise ratio
	＞50db (AGC OFF)

	Video output
	1.0Vp-p,75Ω

	Source
	DC12V±10%

	Power consumption
	≤3W

	Working temperature
	-20℃ ~ +70℃

	Infrared wavelength
	850

	IR LED Quantity
	5

	IR View Distance
	0-3M

	Infrared light on illumination
	0Lux

	Interface
	M12












Product size：
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