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Product feature
1.Exquisite design, exquisite workmanship, precise lines and rigorous structure, reflecting the highest technology; 
2.Integrated structure, shockproof, dust-proof; 
3.ADAS specific camera，suitable for all kinds of vehicles；
4.Adjustable lens angle；
5.Sticker Installation；
6.Dedicated aviation interface design；








Specification
	Model
	MX-ADASH-831A-NNP-025V

	Shell shape
	Plastic shell

	Exterior color
	Black

	Imaging
	1/2.9-inch 1080P CMOS

	Infrared
	\

	Effective pixels
	1920(H)*1080(V)

	Minimum Illumination
	0.01 LUX/F1.2

	Horizontal clarity
	AHD 1080P  

	Scanning frequency
	25Hz

	Audio
	\

	Video output
	1.0V

	White balance
	Automatic

	Shutter
	1/50～1/100000s

	Signal-to-noise ratio
	>46dB

	Current
	Infrared does not activate 65mA/ without infrared

	Voltage
	DC 12V±10%

	Protection level
	IP65

	Working environment
	Temperature -20 º C~75 º C，Humidity -0 º C~90 º C

	Camera angle
	Lens: 6mm，Horizontal: 50 °

	Usage environment
	Inside the car

	Connection connector
	M12 
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