Model:MX-DSMM-838A1-NNP-025H
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Features:
◎ Exquisite design, exquisite workmanship, precise circuit and rigorous structure, reflecting the highest technology;
◎Adjustable bracket, can adjust the angle;
◎ Focus on driver behavior recognition ;
◎Applicable to monitoring in various vehicle environments;
◎Image: positive image/mirror image;
◎Appearance color : black;
◎Specialized aviation interface design.













Specifications:
	Model
	MX-DSMM-838A1-NNP-025H

	Module Type
	FH8535+ 1/4”  GC1084

	resolution
	AHD 720P 

	standard
	[bookmark: _GoBack]PAL

	Total pixels
	PAL:1280(H)×720(V)          

	Minimum illuminance
	0.1LUX

	Electronic Shutter
	1/50 ～ 1/100,000s  

	Signal-to-noise ratio
	> 52dB

	White balance
	Automatic white balance

	Day night switching
	Black and white

	Digital Wide Dynamic
	Open

	Mirror
	Not enabled

	UTC function
	Turn on

	Language
	Default English

	Video output
	1.0Vp-p composite output, 75 Ω

	Lens
	3.9MM, 940 narrowband filter

	Perspective
	Horizontal 50 °

	Interface
	M12 quad core aviation interface (1:+12V, 2: GND, 3: air, 4: video)

	Power supply
	DC 12V±10%

	Operating Temperature
	-20℃～70℃

	Operating Humidity
	Relative humidity below 90%

	Packaging
	Accessory package, certificate of conformity


















Product size:
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