Model: MX-DSMM-839A-NNP-015H
[image: 73ad09c7d8aead17f0770c2c596b73c]
Features:
◎ Exquisite design, fine workmanship, precise circuitry and rigorous structure, reflecting the highest level of technology;
◎  Adjustable stand, allowing for angle adjustment;
◎  Focusing on driver behavior recognition ;
◎  Suitable for monitoring in various vehicle environments;
◎  Appearance color : Black;


Specifications:
	Imaging devices
	ISP: FH8536H
	Sensor: GC2053

	Standard
	AHD PAL

	Effective resolution
	[bookmark: _GoBack]1280 (H) x 720 (V)/1920 (H) x 1080 (V)

	Effective pixels
	720P/1080 P

	Synchronization System
	Internal synchronization

	Vertical synchronization frequency
	50Hz / 60Hz

	Output image
	DMS Black and White

	Video output
	1.0vp-p, 75Ω

	Gamma coefficient
	0.45

	AGC
	automatic

	White Balance
	automatic

	lens
	4.0 mm 

	Lens angle
	Horizontal angle
	80 °

	Effective distance of infrared light
	1-2 meters​​

	IR-CUT
	none

	audio
	none

	Current
	165 mA ± 10% ( DC12V )

	Voltage
	DC 6-16V

	Operating temperature
	- 20 °C~ 70 °C, RH95% MAX

	Storage temperature
	-30°C~80 ° C, RH95% MAX

	Net weight
	182g







Wiring definition:
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Product dimensions:
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