Model：SMART IR PTZ CAMERA
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Features :
· Real-time Monitoring and Remote Control: Allows remote control of camera functions like pan, tilt, and zoom, providing dynamic tracking capabilities via the MDVR's wireless network.
· Comprehensive Coverage: Provides 360-degree surveillance of vehicle interiors and exteriors, covering blind spots and enhancing security.
· Event Recording and Analysis: Captures high-resolution video for post-event analysis, aiding in incident investigation.
· Automated Patrol: Supports preset patrol routes, enabling automated surveillance of specific areas without manual intervention.
· Remote Alarm Integration: Works with sensors to trigger alarms and allows immediate remote viewing for rapid response.
· Robust Data Management: Offers reliable long-term storage and management of high-quality video data.
· Durability: Designed to operate in harsh environments, ensuring stable performance under extreme conditions.
· High scalability: The PTZ camera and MDVR system can add addition cameras and sensors as needed, with expansion interfaces allowing easy future upgrades.
This combination is highly effective in applications such as public transportation, logistics, and law enforcement vehicles, enhancing security, surveillance efficiency, and emergency response capabilities.

Ball machine performance:
	Pan Preset Speed
	300 ° /S

	Tilt Preset Speed
	120 ° /S

	Pan Manual Control Speed
	0 ° -220 ° /S

	Tilt Manual Control Speed
	0 ° -90 ° /S

	Pan Range
	360 ° continuous rotation

	Tilt Range
	90 ° ( 180 ° automatic reverse)

	Preset Point
	256

	Relative Humidity
	90%

	Ingress Protection Rating
	IP66

	Operating Temperature
	-35 ° -+55 °

	Power Input
	DC11V-DC18V

	Weight
	2.5kg
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