Product model: MX-AHDL-D30-NNP-005H
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Features:
◎ Exquisite design, exquisite workmanship, precise circuit and rigorous structure, reflecting the highest technology;
◎ Equipped with dual camera modeling and detection function ;
◎Meet the needs of most passenger vehicles;
◎Image: positive image/mirror image;
◎Appearance color: black;
◎Specialized aviation interface design;

Parameters and specifications:
	model
	MX-AHDL-D30-NNP-005H

	Image Sensor
	 1/3 CMOS

	Video format
	PAL (PAL or NTSC optional)

	Horizontal resolution
	700TVLines

	Image Output
	Synchronous sampling output

	Lens spacing
	5cm (12cm is selected according to the detection range)

	Lens parameters
	 960×576 pixels, 2.8mm(2.1mm/2.8mm/3.6mm/4mm/6mm/8mm optional)

	White Balance
	Automatic white balance

	shutter
	1/50-1/80000 (seconds) 1/60-1/80000 (seconds)

	Frame rate
	25 fps

	Video output interface
	Composite video output, aviation head interface

	Gain
	Automatic Gain Control

	Signal-to-Noise Ratio
	＞48db

	power supply
	12V voltage input

	power
	≤2W

	size
	165×59.65×68mm (L×W×H)

	weight
	About 0.35KG

	Operating temperature range
	-20～+70℃

	Relative humidity
	[bookmark: _GoBack]10%～90% non-condensing

	Heat dissipation
	No active heat dissipation, passive structural heat dissipation

	Field of view
	2.8MM Horizontal: 105° Vertical: 60°



Dimensions:
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