Product model：M22-NNNN
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Features:
◎ Exquisite design, exquisite workmanship, precise circuit and rigorous structure, reflecting the highest technology;
◎ Equipped with dual camera modeling and detection function ;
◎Meet the needs of most passenger vehicles;
◎Image: positive image/mirror image;
◎Appearance color: black;
◎Specialized aviation interface design;











1. System parameters

	project
	Equipment parameters
	illustrate

	
	Kernel system
	L inux

	system
	Operating language
	Chinese, English, Spanish (other languages can be customized)

	
	User interface
	C/S operation configuration method

	
	Operating mode
	Remote control, computer client, web





2. Video parameters

	project
	Equipment parameters
	Indicators

	
	Image sensor
	1/3 CMOS​

	
Images and videos

	Video format
	PAL or NTSC standards (optional)

	
	Horizontal resolution
	700 TV Lines

	
	Preview function
	Single-channel, two-screen splicing;

	
	Video output
	1-channel video output (CVBS)

	
	OSD
	Images overlaid with information such as time, date, and passenger flow.

	
	Compression format
	H.264​

	
	Lens parameters
	960*576 pixels, 2.8 mm (2.8mm/3.6mm/4mm/6mm optional)

	
	Resolution
	D1



3. Alarm parameters

	project
	Equipment parameters
	Indicators

	Call the police
	Enter
	Two alarm I/O inputs, configurable for low-level alarms below 1V or high-level alarms above 4V .

	
	Functional alarm
	Video loss, video obstruction, overload alarm



4. Communication interface

	project
	Equipment parameters
	Indicators

	Communication interface
	RS485 interface
	One RS485 interface, supporting protocol integration and custom protocol development.

	
	RJ45
	One RJ45 interface, which can be used for testing, copying, setting, recording, upgrading, and transmission.



5. Electrical parameters

	project
	Equipment parameters
	Indicators

	
Power supply and power consumption

	Power input
	8V～36V. Please ensure your vehicle's power supply is within this range before use. Prolonged use above 36V will damage the machine.

	
	Power on/off
	Supports AC boot and delayed shutdown.

	
	ACC
(Car key signal)
	≤4 V
	Power off

	
	
	≥5 V
	Power on

	
	Output voltage
	+12 V @0.5 A

	
	Power
Consumption
	Normal operating conditions <4 W

















6. Other parameters

	project
	Equipment parameters
	Indicators

	
Other
	Work environment
	Temperature
	-20 ℃ ~ 70 ℃

	
	
	Humidity
	10 % ~ 90 % (non-condensing)

	
	Heat dissipation
	No active cooling, using passive structural cooling.

	
	Size
	[bookmark: _GoBack]133X50X59.65mm (excluding mounting bracket)

	
	Total weight
	Approximately 0.45 kg​

	
	Statistical precision
	> 95 %




7. Specifications and dimensions
[image: ]




image1.jpeg




image2.png
o

k N )

‘ ®
o




