Product model: MX-AHDX-TA4
[image: ]

Features:
◎ Exquisite design, exquisite workmanship, precise circuit and rigorous structure, reflecting the highest technology;
◎The lens is adjustable, and the angle can be adjusted at will during the installation process;
◎Long viewing distance and wide viewing angle;
◎Waterproof sealed aluminum cover, using special waterproof treatment materials, reaches IP66 waterproof effect, suitable for outdoor use;
◎Integrated structure, shockproof and anti-loosening design;
◎Suitable for monitoring in various vehicle environments;
◎Image: positive image/mirror image;
◎Appearance color: white.

Specifications:
	Specification
	Power supply (optional)
	DC12V I in ≥4A

	
	Power consumption
	35W

	
	weight
	7Kg

	
	Installation
	Flat base installation

	
	Relative humidity
	10-90%

	
	Operating temperature
	-35℃~55℃

	
	Waterproof grade
	IP66

	
	Aperture & Zoom
	Automatic/Manual

	Basic functions of PTZ
	Horizontal rotation
	100°/S max

	
	Rotate up and down
	60°/S max

	
	Preset position
	Up to 256

	
	Patrol function
	support

	
	Line scan speed
	0.5～30°/s

	Infrared light
	Infrared emitter
	High brightness LED array x 7

	
	wavelength
	850nm

	
	Throw distance
	100 meters

	
	Power consumption
	10W

	
	Infrared light control
	Automatic/menu manual control

	
	Infrared lamp life
	More than 20,000 hours




Specifications and dimensions:
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