PTZ--Relay connection
As following:
[image: 1dc844062bc12ac7c6fe6a2cda94aa8]

Connection
[image: b144cd463bf759037bb4984d2532d1f]


Description：

1. The 85 and 86 pins of the relay are respectively connected to the negative pole of the car fuse box/the negative pole of the pan/tilt power cord and the ACC ignition switch.
2. The 30-pin of the relay is connected to the normal power of the car.
3. [bookmark: _GoBack]The 87a of the relay is connected to the positive pole of the power cord of the gimbal.
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