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Product introduction
M15Hv is a high-performance, high- expansion product specially developed for in-vehicle video surveillance and remote video surveillance. etc. technology. M15Hv has a compact structure, elegant appearance, and easy installation and use. It is a basic product for lightweight applications. It is suitable for public safety, long-distance passenger transportation, road inspection and other automotive mobile monitoring fields.
Product advantages
· The in-vehicle interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 optional
· [bookmark: _GoBack]Support 4G , GPS function module
· Support one SD card
· Abundant peripheral interfaces
· Support external UPS battery life
· High scalability







Core parameters
	Project
	Parameter Description

	Audio and video input
	AHD video input
	External 4 * 1080P

	
	Video standards
	30FPS

	
	Audio Input
	2

	Audio and video output
	CVBS output
	1

	
	VGA output
	1 (optional)

	
	Audio output
	1

	Audio and video parameter encoding
	Video encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	
	Audio coding
	G.711A

	Storage Space
	SD card
	1 , maximum 1T

	Wireless network
	4G wireless
	1 SIM card

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	Interface
	USB
	1​

	
	RS232
	1 group

	
	RS485
	1 group(optional)

	
	SENSOR
	4

	
	SENSOR OUT
	1

	
	NET
	1 (optional)

	Physical specifications
	Size
	102.8mm ( L ) *120mm ( W ) *32.23mm ( H )
(excluding tail wire)

	
	Weight
	NW：0.6kg，GW：0.8kg
 ( with a fluctuation of 5% )

	Work Environment
	Operating temperature
	-20 ～ +70 ℃

	
	Operating humidity
	8% ~ 90% (no condensation)

	Other
	Operation Mode
	Remote control, mobile phone APP , WEB








Product Size
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Unit: mm
Panel interface
front panel
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rear panel
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tail line definition
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