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Product Introduction
M18Ev is a car mounted device that adopts an integrated structure. The device comes with one front facing camera and integrates 4G, WIFI, GPS, GSENSOR and other modules internally. Equipped with a 1080P high-definition camera, it is both convenient and secure.


Product advantages
· Video encoding H.265 and H.264 are optional
· Built in 4G, WIFI, GPS function modules
· Supports 2 TF card
· Comes with 1 built-in camera
· Equipped with adhesive surface, supporting quick installation









Core parameters
	Project
	Parameter Description

	Audio and video input
	Video Input
	Built-in: 1*1080P
External: 3*1080P AHD/1*1080P IPC (optional)

	
	Built-in camera perspective
	D:130°H:105°V:53°

	
	Video Standards
	30FPS

	
	Audio Input
	built-in

	Audio and video output
	CVBS output
	Support

	
	Audio Output
	Built-in

	Audio and video parameter encoding
	Video Encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	
	Audio Coding
	G.711A

	Storage Space
	TF card
	2, maximum 1T*2

	Wireless network
	4G Wireless
	1 SIM card

	
	WIFI
	2.4G

	Positioning method
	BeiDou/GPS
	Support, mixed positioning possible

	interface
	RS232
	1 group

	
	SENSOR
	1 (optional)

	
	SENSOR OUT
	1 (optional)

	
	ADC
	1 (optional)

	Physical specifications
	Size
	110mm (L)*70.5mm (W)*35.6mm (H)

	
	Power cord
	Length 2m, diameter 5.1mm

	
	Video cable
	3 (optional), 3m long, 3.5mm in diameter

	
	Weight
	NW: 0.22kg，GW: 0.62kg
(with a fluctuation of 5%)

	Work Environment
	Operating temperature
	-20～+70℃

	
	Operating humidity
	8%～90% (no condensation)

	Other
	Power Management
	Switch button

	
	G SENSOR
	Support

	
	Linkage alarm
	Acceleration, rollover, collision trigger

	
	Power consumption
	≈4W
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