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MDVR-M19Ev

( RFID version )

Product Introduction
The M19Ev series features an integrated design, incorporating front and rear dual cameras, 4G, Wi-Fi, and GPS. While the rear camera records the vehicle's interior environment, the front camera simultaneously records road conditions, offering significant advantages in convenience and safety. The M19Ev series supports mainstream technologies such as H.265 video encoding and GPS/BD hybrid positioning. Optional features include rapid detection and collision detection, making it suitable for onboard or remote monitoring environments in freight vehicles, passenger buses, construction vehicles, sanitation vehicles.




Product Advantages
· Specialized vehicle interface ensures reliable and stable operation in complex environments.
· Video encoding options: H.265 or H.264
· Built-in 4G, WIFI, and GPS modules
· Supports two Micro-SD (TF) cards .
· Built-in front and rear dual cameras
· It has an adhesive side and supports quick installation.
· RFID support (optional)













Core parameters
	Project
	Parameter Description

	Audio and video input
	Video input
	Built-in 2* CMOS 1080P cameras ( front and rear dual view )

	
	Forward focal length
	[bookmark: OLE_LINK4][bookmark: OLE_LINK3]3.0MM

	
	Forward view
	HFOV=111° VFOV=59° DFOV=133°

	
	Intraocular focal length
	2.1MM

	
	Inner vision
	HFOV=130° VFOV=73° DFOV=160°

	
	Audio input
	Built-in 1 microphone

	Audio and video output
	Audio output
	Built-in 1-channel speaker

	Audio and video parameter encoding
	Video encoding
	H.265/ H.264

	
	Video resolution
	[bookmark: _GoBack]1080P/720P/D1

	
	Audio encoding
	G.711A

	Storage space
	TF card
	2 cards, maximum 512GB *2

	Wireless network
	4G wireless
	1 SIM card

	
	WIFI
	2.4G

	Positioning method
	BeiDou/GPS
	Supports mixed positioning

	interface
	RS232
	Group 1

	
	Sensor
	1
High-level alarm: 3.3~36V / Low-level alarm: 0~3.3V

	
	Sensor out
	1

	
	ADC
	1 (Analog input, optional)

	Physical Specifications
	Size
	123.6mm (L)*80.5mm (W)*47.7mm (H)

	
	Weight
	NW: 225g
GW : 400g (M19Ev standard version)

	Work environment
	Operating temperature
	-20 to +70℃

	
	Operating humidity
	8%~90% (non-condensing)

	other
	RFID
	Built-in card swiping function (ISO15693 protocol , optional )

	
	Collision sensing
	Post-parking collision detection

	
	Gravity sensor
	Built-in GSensor

	
	Linked alarm
	Alarms triggered by acceleration, rollover, and collision.




Product Dimensions
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