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M D VR-M25Hv

	Note: The appearance of the device may vary slightly depending on the version.	
 
 
Product Introduction
The M25Hv series is designed for in-vehicle video surveillance, intelligent image recognition, and highly expandable products. It utilizes the high-speed NT98321 processor and an embedded operating system, integrating cutting-edge IT technologies such as H.264/H.265 video compression / decompression. Its multi-functionality allows for diverse product development, such as: a 4- channel video splitter, a 4- channel BSD intelligent recognition alarm, and a DMS ( Driver Fatigue Assist System).

Product Advantages
· Supports up to 4 AHD video inputs
· Video encoding options : H.265 or H.264
· Supports AHD 1080P output.
· Supports one TF card
· Abundant peripheral interfaces
· High scalability
















Core parameters
	project
	Parameter Description

	AI Functions
	ADAS, DSM, BSD
	Full-featured AI

	Video input
	AHD input
	External 4 * 1080P

	Audio and video output
	AHD output
	Route 1 ( 1080P )

	
	Voice output
	1 ( four-core male connector，yellow )

	Video parameter encoding
	Video encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	Storage space
	TF card
	1, maximum 1TB

	Interface
	RJ45
	1 ( 100MB )

	
	RS232
	1( GPS module )

	
	SENSOR OUT
	1

	
	M12 4-core aviation female connector (V)
	4
​( 4- channel AI video input )

	
	M12 4-core aviation male connector (V)
	1( AHD video output )

	
	M12 4-core aircraft carrier bow ( A )
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( For external speaker output )

	Physical Specifications
	Size
	1 30 mm (L) * 71.2 mm (T) * 27.8 mm (H) 

	
	Weight
	GW：0.3kg; NW：0.34kg

	Work environment
	Operating temperature
	-20 to +70℃

	
	Operating humidity
	8%~90% (non-condensing)

	other
	Operating mode
	Mobile App, Web








Dimensions
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