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Product introduction
[bookmark: _GoBack]M32Hv series is a dedicated vehicle-mounted audio and video surveillance product that uses a high-speed processor. It adopts a waterproof and dustproof structural design and an embedded operating system, integrating IT cutting-edge technologies such as H.264/H.265 video compression / decompression, 4G network, GPS/BD positioning, etc. It has the characteristics of strong earthquake resistance, simple appearance, flexible and convenient installation, comprehensive functions, and high reliability. 
Product Advantage
· The interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 is optional
· Support 4G 、WIFI and GPS functional modules
· Supports a 2.5-inch optional SSD/HDD hard disk
· Support two SD cards
· Rich peripheral interfaces
· Support external UPS battery life
· Waterproof dust-proof








Core parameters
	Project
	Parameter Description

	Audio and video input
	AHD Video Input
	External 4 * 1080P

	
	Video Standards
	30fps

	
	Audio Input
	4+1

	Audio and video output
	CVBS output
	1

	
	VGA output
	1 (optional)

	
	Audio Output
	1

	Audio and video parameter encoding
	Video Encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	
	Audio Coding
	G.711A

	Storage Space
	Solid State Drive
	1, maximum 8TB

	
	SD Card
	2 sheets , maximum 1T*2

	Wireless network
	4G Wireless
	1 SIM card

	
	WIFI
	2.4/5.8G ( optional)

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	Interface
	RS232
	1 group

	
	RS485
	1 group (enhanced version)

	
	SENSOR
	2/4 (Enhanced Edition)

	
	SENSOR OUT
	2 (Enhanced version)

	
	ADC
	2 (Enhanced version)

	
	USB
	1 ( Enhanced version)

	
	NET
	1 (Enhanced version)

	
	MIC
	1

	Physical specifications
	Size
	154mm ( L ) *148mm ( W ) *39mm ( H )
(excluding tail wire)

	
	Weight
	NW：1.10 kg，GW：1.40 kg 
(fluctuating 5% up and down)

	Work Environment
	Operating temperature
	-20°C to +70°C

	
	Protection level
	10% ~ 95% (no condensation)

	
	Protection Rating
	IP66

	Other
	Operation Mode
	Remote control, APP , WEB

	
	G SENSOR
	support
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