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Product introduction
M51/52Hv is designed for vehicle video monitoring, remote video monitoring development of a high-performance, highly expandable product, featuring a self-ejecting hard drive structure and high-speed processor NT98323 and embedded operating system, integration of IT cutting-edge field H.264/H.265 video compression or decompression, 4G network, GPS/BD positioning technology. It has the characteristics of strong earthquake resistance, simple appearance, flexible and convenient installation, comprehensive function and high reliability. 







Product Advantage
· The interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 is optional
· Support 4G WIFI and GPS functional modules
· Supports a 2.5-inch optional SSD/HDD hard disk
· Supports one SD card
· Rich peripheral interfaces
· Support external UPS battery life
· High scalability












Core parameters
	Project
	Parameter Description

	Audio and video input
	AHD Video Input
	M51Hv external 4 * 1080P
M52Hv external 8*1080P

	
	Video Standards
	30FPS (4 channels) / 15FPS (8 channels)

	
	Audio Input
	5

	Audio and video output
	CVBS output
	1

	
	VGA output
	1(optional)

	
	Audio Output
	1

	Audio and video parameter encoding
	Video Encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	
	Audio Coding
	G.711A

	Storage Space
	Harddisk
	SSD/HDD, maximum 8T

	
	SD Card
	1 card, maximum 1T

	Wireless network
	4G Wireless
	1 SIM card

	
	WIFI
	2.4/5.8G ( optional)

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	Interface
	RS232
	1 group

	
	RS485
	1 group

	
	SENSOR
	4

	
	SENSOR OUT
	2

	
	ADC
	2

	
	USB
	1

	
	NET
	1

	
	MIC
	1

	Physical specifications
	Size
	176.9mm ( L ) *186.8mm ( W ) *54mm ( H )
(without cable shroud)

	
	Weight
	NW：1.4kg，GW:2kg​
(fluctuating 5% up and down)

	Work Environment
	Operating temperature
	-20 ～ +70 ℃

	
	Operating humidity
	8% ~ 90% (no condensation)

	Other
	Operation Mode
	Remote control, APP , WEB

	
	G SENSOR
	Support




Size
[image: C:\我的乱七八糟\真乱七八糟\51h.png]
Panel& interface
[image: d:\Documents\Tencent Files\280646473\Image\C2C\Image1\@2Y9_5HS[{GSO@SIK[({5WP.png]
Front panel
[bookmark: _GoBack][image: d:\Documents\Tencent Files\280646473\Image\C2C\Image1\@AD1LRZP6W}F_W7$CK{_]BU.png]
Rear panel

image5.png
DC 8-36V

1NO AV
NV

Z NI AV

L NIA/VY





image2.png




image3.png




image4.png
147 sim





image1.png
‘N BIRERES%
CITOPS




