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Product Introduction
The M71Hv portable video transmission system is a highly portable and extensible product developed for drone monitoring, capturing, command, and HDMI-based ultra-high-definition video transmission. The product features an integrated industrial design, incorporating hardware audio-video encoding, 5G/4G networks, GPS & BeiDou positioning, data storage, and lithium battery modules. It can connect to drones, robots, and DV cameras via an HDMI interface, enabling the management end to remotely access ultra-clear real-time video from the operation site.




Product Advantages
· IP65 protection level, suitable for various complex environments
·  Video coding H.265, H.264 optional
·  Support 5G, 4G, WIFI, GPS function modules
·  Support a MicroSD (TF) card storage
·  Built-in lithium battery, continuous work for 8 hours
· [bookmark: _GoBack] Support two-way intercom and cluster intercom;
· Comes with an anti-glare status display
· Comes with USB, HDMI and other interfaces
· High scalability






Core Parameters
	project
	Parameter Description

	Audio and video input
	AHD Input
	1

	
	HDMI input
	1

	
	Audio Input
	1  (Bluetooth)

	
	Wired MIC
	support

	Audio Output
	Voice Output
	1  (Bluetooth)

	
	Wired headphones
	support

	Audio and video parameter encoding
	Video Encoding
	H.264/H.265

	
	Video resolution
	1080P/720P

	
	Audio Coding
	G711A , G711U , AAC

	Storage Space
	TF card
	1 sheet, maximum 1T

	Wireless network
	5G/4G Wireless
	2 SIM cards​
( With built-in 5G or 4G card access port , supports 1.4G private network)

	
	WIFI
	WiFi Client connection / WiFi AP hotspot

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	power supply
	Battery capacity
	7.4v 6000mAh lithium battery pack

	
	Power Management
	Key switch , automatic screen saver

	
	Type-C charging
	Support (current >2A )

	
	Magnetic charging
	support

	Screen
	OLED screen
	1.54 inches

	
	show
	Positioning, network, power, time

	button
	SOS button
	1

	interface
	External AHD
	1 ( 4- core M6 aviation connector )

	
	TYPE-C
	Charging / network port

	
	Mini HDMI
	1

	Physical specifications
	size
	149mm ( L ) *98.1mm ( W ) *42.6mm ( H )
(without antenna, back clip)

	
	weight
	NW 0.74 kg ( up or down 5%)

	Work Environment
	Operating temperature
	-20 ～ +6 0 ℃

	
	Operating humidity
	8% ~ 90% (no condensation)

	other
	Remote Control
	PC , APP​

	
	Support Agreement
	GB28181 , private protocol
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