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Product introduction
4G HD IR PTZ Camera is a professional HD IR PTZ camera integrated with record, HD video wireless transmit, audio ,talk and remote control. It adopts high speed processor hardware and embedded Linux system. The state of the art HD camera use the latest IT technologies, such as H.265 code, wireless transmitting technologies, remotely control etc. 


Product advantages
· The in-vehicle interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 optional
· Support 4G /5G , GPS function module
· Support one SD card
· Abundant peripheral interfaces
· Support external UPS battery life
· High scalability







Core parameters
	project
	Parameter Description

	Video Parameters
	IPC Input
	1st Road

	
	CVBS output
	1 (built-in)

	
	Video Encoding
	H.264/H.265

	
	Video resolution
	Maximum 4K (optional)

	
	Support Agreement
	GB28181 , private protocol

	Audio parameters
	Audio Input
	Bluetooth hand tag/built-in MIC

	
	Audio Output
	Bluetooth Hand Tag

	
	Audio Coding
	G.711A

	storage
	SD Card
	2 sheets, maximum 512G*2

	Positioning method
	BeiDou/GPS
	Support, mixed positioning possible

	network
	4G
	1/2 SIM cards (optional)

	
	WIFI
	2.4G

	
	RJ45
	1st Road

	Call the police
	I / O
	1 channel (optional)

	PTZ
	Horizontal range
	360° rotation

	
	Horizontal speed
	120°/s

	
	Vertical Range
	-15° - 90°

	
	Vertical speed
	60°/s

	
	Preset Point
	200

	power supply
	Power
	Daytime work ≈ 15 hours / Nighttime work ≈ 10 hours
Can be powered by external power supply

	
	Power Management
	Switch button

	Physical specifications
	size
	170mm(W)*277mm(H)*170mm(D)

	
	Bracket height
	1330mm

	
	weight
	[bookmark: _GoBack]NW: 4.3kg GW : 11.3kg
( with a fluctuation of 5% )

	Work Environment
	Operating temperature
	-25℃～+60℃
(Ambient temperature under well-ventilated conditions)

	
	Operating humidity
	10%～95% (no condensation)

	other
	Installation Mode
	Comes with bracket/ chassis magnet adsorption

	
	Protection level
	IP66






Product Size
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Unit: mm
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