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Product Introduction
The M91Sv lightweight MINI surveillance ball is a wireless video application integrated product with comprehensive functions, easy installation and use. It has the characteristics of high integration, large-capacity lithium battery pack, waterproof and shockproof, and MINI size. The bare weight is only 1.4KG , which can be carried around and meets the special requirements of temporary rapid surveillance and remote dispatching and command. 
Product Advantages
· Lightweight design
· IP6-5 protection level
· Voice intercom function
· Built-in large-capacity battery, long-lasting work
· 360 ° PTZ control
· Support 4G , WIFI
· Support wired network port







Core parameters
	project
	Parameter Description

	Video Parameters
	IPC Input
	1

	
	Optical zoom
	Maximum 10 times

	
	Night vision distance
	30m

	
	Video Encoding
	H.264/H.265

	
	Video Pixels
	Maximum 2K (optional)

	
	Support Agreement
	GB28181. Private protocol

	Audio parameters
	Audio Input
	built-in

	
	Audio Output
	built-in

	Storage
	TF card
	1 , maximum 1T

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	network
	4G/5G
	1 piece

	
	WIFI
	2.4G

	
	Wired network port
	1 channel (optional)

	Call the police
	I/O
	1 channel (optional)

	PTZ
	Horizontal range
	360° continuous rotation

	
	Horizontal speed
	120°/s

	
	Vertical Range
	-15° - 90°

	
	Vertical speed
	60°/s

	
	Preset Point
	200

	power supply
	Power
	[bookmark: _GoBack]5000mAh , 11.1V lithium battery pack

	
	Working hours
	during the day: 10 hours
Night time: 6 hours

	
	Power Management
	Switch button

	
	Charging Mode
	USB ( 2A ) / Power Bank

	Physical specifications
	size
	102.4mm ( W ) *188mm ( H ) *85mm ( D )

	
	Bracket height
	Maximum height including bracket : 1.7m

	
	weight
	NW: 1.4KG, GW: 2.7KG
(The remaining floating rate is 5%)

	Work Environment
	Operating temperature
	-25℃～+60℃
(Good ventilation environment)

	
	Operating humidity
	10%～95% (no condensation )

	other
	Installation Mode
	Comes with bracket/ chassis magnet adsorption

	
	Protection level
	IP65





Movement parameters
   Movement parameters are configured according to the specific model of the equipment. If necessary, please inform our company of your actual technical requirements for assistance.
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