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Product Introduction
The M9 2 Sv lightweight mini surveillance PTZ camera is a comprehensive, portable, and easy-to-install wireless video application product. It features high integration, a large-capacity lithium battery, waterproofing and shockproof design , and a miniature size, weighing only 2.5 kg , making it easily portable and meeting the special requirements of temporary rapid deployment and remote dispatching. 


Product Advantages
· Lightweight design
· IP6 protection rating
· Voice intercom function
· Built-in high-capacity battery for long-lasting operation
· 360 ° omnidirectional PTZ control
· Supports 4G and WIFI
· Supports wired network ports
· Supports NARI encryption








Core parameters
	project
	Parameter Description

	Video parameters
	Video input
	1-channel IPC input

	
	Optical zoom
	Maximum 10 times

	
	Night vision distance
	30 meters

	
	Video encoding
	H.264/H.265

	
	Video pixels
	The default maximum is 2K ( optional ) .

	
	Support Agreement
	GB2818 1. Private Protocol

	Audio parameters
	Audio input
	Built-in microphone

	
	Audio encoding
	G.711A, G.711U, PCM

	
	Audio output
	Built-in speaker

	Storage method
	TF card ( standard version)
	1 sheet, maximum 1TB

	
	Dual SIM (NARI version)
	Enabling the NARI encryption function allows for the addition of one more TF card .

	Positioning method
	BeiDou/GPS
	Supports mixed positioning
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	4G/5G ( Standard Version)
	One 4G/5G SIM card (compatible with all networks )

	
	Optional 4G card (NARI version)
	NARI Encrypted Network: Supports one 4G SIM card compatible with all network types (optional)

	
	WIFI
	WIFI 6 (backward compatible with 5.8/2.4G )
Supports STA/AP modes

	
	Wired network port
	Route 1

	Call the police
	I/O
	One input/one output (selectable, optional)

	Gimbal
	Horizontal range
	360° continuous rotation

	
	Horizontal speed
	120°/s

	
	Vertical range
	-15°-90°

	
	Vertical velocity
	60°/s

	
	Preset point
	200

	power supply
	Built-in battery
	11.1V 10000mAh Lithium Battery Pack

	
	Working hours
	Daytime ≈ 20 hours/Nighttime ≈ 12 hours

	
	Power Management
	switch button

	
	Charging mode
	Desktop adapter (4A ) , M12 aviation connector (7 pins)

	Physical Specifications
	size
	150mm ( W ) * 250.8mm ( H ) * 99mm ( D )​​​

	
	bracket height
	Maximum height including bracket : 1700mm

	
	weight
	NW: 2.5KG, GW: 8KG (fluctuation within 5%)

	Work environment
	Operating temperature
	-25℃ to +60℃ (in well-ventilated environments)

	
	Operating humidity
	10%–95% (non-condensing )

	other
	Installation mode
	Comes with a built-in bracket/base magnetic attachment.

	
	Protection level
	IP6 6




Movement parameters
   The movement parameters vary depending on the specific model of the equipment. If needed, please inform our company of your actual technical requirements for assistance.
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