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Product Introduction
M93H 4G camera is a comprehensive, lightweight, and easy-to-install wireless video application product. It features high integration, waterproof and shockproof design, simple installation, and meets the specific requirements of rapid deployment and remote dispatching. It is suitable for business scenarios such as construction site monitoring, vehicle surveillance, and theft prevention. The AI version also supports functions such as facial recognition, blind spot personnel detection, and driver fatigue warning.




Product Advantages
· Integrated design
· IP66 protection rating
· Equipped MIC-Online intercom
· Wide voltage supply
· Supports 4G , BD/GPS
· Supports multiple application platforms
· Supports video AI functions













Core parameters
	project
	Parameter Description

	Video parameters
	Built-in Input CMOS
	1080P 25/30fps

	
	Infrared night vision
	Automatic color-to-black switch at a distance of 10 meters.

	
	Extended input video
	External AHD 1080P input is available (optional).

	
	Video output
	AHD 720P/1080P output (optional)

	
	Lens parameters
	Default 2.8mm (View angle 105 °)

	Audio parameters
	Audio input
	Built-in microphone (optional)

	
	Audio output
	Built-in speaker

	Storage method
	TF card
	1 sheet, maximum 512GB

	Positioning method
	BeiDou/GPS
	Supports mixed positioning

	Network
	4G
	Supports all network compatible 4G cards

	
	WIFI
	No

	Interface
	Alarm input
	1-channel ADC input(optional)

	
	Alarm output
	1-channel controllable 10V voltage output(optional)

	
	RS232
	Supports one RS232 input (optional)

	Power supply
	Input voltage
	8-36V

	
	Output voltage
	10V (optional)

	
	Power Management
	ACC power on/off, alarm input triggers power on/off

	
	Power connection method
	Vehicle power supply and adapter, can be equipped with a dedicated UPS (plug and play, can work for 18 hours on a full charge).

	
	Power consumption
	Standalone version: 1.9W during the day, 3.5W at night.

	Intelligent algorithms
	Dysfunction Driving Management System (DSM)
	Facial recognition, closing eyes, yawning, making a phone call, smoking, looking left and right (optional)

	
	Blind spot monitoring BSD
	Personnel intrusion detection (optional)

	
	Advanced Driver Assistance Systems (ADAS)
	Lane departure warning, forward collision warning, and vehicle in front starting (optional)

	
	License plate recognition
	Supports license plate recognition, image capture, and uploading.(optional)

	[bookmark: _Hlk211072236]Physical Specifications
	Size
	77.5 mm ( W ) * 61 mm ( H ) * 74 mm ( D )

	
	Bracket height
	23.5mm

	
	Weight
	NW:0.42KG 
(Fluctuation within 5%)

	Work environment
	Operating temperature
	-20℃ to +70℃
(Good ventilation environment)

	
	Operating humidity
	10%–95% (non-condensing )

	Other
	Installation mode
	Comes with stand

	
	Protection level
	IP66



Note : The AI algorithm can only support one set at a time.






Interface Description
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Dimensions
[bookmark: _GoBack][image: 123][image: ]
[image: ][image: ]

image3.png




image4.png
82.573





image5.png
M4X6 64+





image6.png




image7.png
N

) o/ (]

RINEvEA)

R3, 4+
3. 20




image2.png




image1.png
‘N BIRERES%
CITOPS




