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Core parameter
	Item
	Introduction

	Power
	power input，GND
	5~12V

	Communication interface
	RS232
	1 set

	
	RS485
	1 set

	Communication mode
	Two-way communication

	Size
	4.7(L)*2(W)*1(H) cm

	Wire length
	RS232
	19.5 cm

	
	RS485
	19.5 cm

	Wire harness
	power input
	red，Casing text：12V/5V

	
	GND
	black，Casing text：GND

	
	RS232 RX
	white，Casing text：RX

	
	RS232 TX
	yellow，Casing text：TX

	
	RS485A
	yellow，Casing text：RS485A

	
	RS485B
	white，Casing text：RS485B
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