Multil- functional Mic
Model：MX-HMC-02
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Product parameters
	Item
	Description

	Video/Audio
	Receiving sensitivity
	0.25μV

	
	Rated audio
	500mW

	
	Spurious suppression
	70dB

	
	Audio response
	+1~-3dB

	General
	Working voltage
	5-12V

	
	Water and dust resistant
	IP54

	
	Operating temperature
	-30℃~+60℃

	
	Size(H*W*D)
	82*58*40mm







Product size
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Installation matters
· Pins definition
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	NO.
	function
	describe

	1
	Power
	5-12V/200mA

	2
	GND
	GND

	3
	RS232 RX  
	RX1

	4
	[bookmark: _GoBack]RS232 TX
	TX1

	5
	MIC
	IN

	6
	SPK
	OUT
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