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parameter
	Item
	Parameters

	[bookmark: _GoBack]Environment temperature
	-25℃～+70℃

	Dielectric Strength
	AC250V (50Hz for 1mi nute)

	Rating
	DC12V. 50mA

	Electrically Life
	100. 000Cycles

	Contact Resistance
	≤30m0

	Travel
	0.2士0.05mn

	Insulation Resistance
	≥100MO

	Actuating Force
	100 -350gf

	Relative Humidity
	(40C)≤95%








size drawing
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product component
	Name
	Model
	Color
	Materials
	Quantity
	Size

	Injection moulding
	Push-button alarm switch
	black
	PVC
	1
	

	Switch
	Reset switch
	black
	PA66
	1
	

	Follow-up material specifications
	2468 2pin
	Black
	PVC
	1
	5ooMM
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Circuit Diagram
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