Model: MX-AHDH-110B-ANP-015,2.8mm  
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Product feature
1. Exquisite design, exquisite workmanship, precise lines and rigorous structure, reflecting the highest technology; 
2. Dedicated 3M superglue design；
3. Integrated structure, shockproof, dust-proof, anti-fog design; 
4. Suitable for all kinds of vehicles；
5. Image: positive/mirror image；
6. Color: black;
7. Dedicated aviation interface desig-110A/BMW CIC head-110B；

Specifications:
	Project
	Parameter

	Model
	MX-AHDH-110B-ANP-015,2.8mm

	Chip
	[bookmark: _GoBack]1/2.9″ CMOS 

	Resolution
	1080P AHD

	Signal system
	PAL

	Image source
	AHD

	Pixel
	1920(H) x 1080(V)

	Shot
	2.8mm

	Horizontal angle
	100°

	Minimum illumination
	0Lux

	Backlight Compensation
	built-in

	Shutter speed
	1/53~1/100,000（S）

	Interface
	BMW head interface

	White balance
	automatic tracking

	Signal to Noise Ratio
	>50db (AGC OFF)

	Video output
	1.0Vp-p,75Ω

	Power supply
	DC12V±10%

	Operation temperature
	-20℃ ~ +70℃

	Size
	58mm*34mm*71mm
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