Product Model: MX-AHDH-266A-NNP-005H
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Features:
◎ 1/2.9″ high-resolution CMOS sensor
◎ 1080P Ultra HD Camera
◎ Supports automatic white balance
◎ Supports low-light night vision down to 0.01 Lux
◎ Horizontal angle of the lens: 165°
◎ Compact design supports better waterproofing 
◎ Multiple mounting holes for quick installation
◎ Appearance color: Black;























Specifications:
	Model
	MX-AHDH-266A-NNP-005H

	plan
	FH8536+2053

	Image sensor
	1/2.9″ CMOS AHD

	Resolution
	1080P

	Signal System
	PAL system

	Pixels
	1920 (H) x 1080 (V)

	lens
	1.58mm lens

	Horizontal
	165°

	Minimum Illumination
	0.01 Lux

	Backlight compensation
	automatic

	Shutter speed
	Automatic: 1/50 to 1/100,000 (seconds)

	White Balance
	Automatic white balance tracking

	Wide dynamic range
	none

	Signal-to-noise ratio
	Greater than 55dB (AGC OFF)

	Video output
	1.0Vp-p, 75Ω

	power supply
	DC12V±10%

	Power consumption
	≤3W

	Operating temperature
	-20℃ ~ +70℃

	Infrared wavelength
	/

	Number of infrared lights
	/

	Infrared light illumination distance
	/

	Infrared light illuminance
	/
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	M12 aircraft carrier bow (with O-ring)

	External dimensions
	41*40*31 (mm)
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