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Product features:
1. Low power consumption, easy dissipate heat;
2. Good color reduction and picture quality;
3. Mini conch construction, Exquisite, beautiful and fashion;
4. High hardness, Anti-collision;
5. Built in imported 12 pcs Φ5 IR LED lights, 5m shooting distance;
6. Infrared function auto on when light lower than 10Lux;
7. Use imported lens plate, good moisture-proofing;
8. Color: gray;
9. Appropriative aviation connector design;











Specifications:
	Model
	MX-AHDH-301A-NNP-005H

	Image sensor
	1/2.9” Aptina 0130 with Nextchip2431

	Resolution
	1080P/720P

	Signal system
	PAL/NTSC

	Pixel
	PAL/NTSC：1920（H) x 1080(V)/1280（H) x 720(V)

	Lens
	Standard 2.8mm/3.6mm lens

	Horizontal angle of view
	105°/80°

	Minimal illumination
	0Lux

	Backlight compensation
	Built-in

	Shutter speed
	1/53~1/100,000 sec

	White balance
	Automatic tracking

	Noise-signal ratio
	＞50db (AGC OFF)

	Video output
	1.0Vp-p,75Ω

	Power
	DC12V±10%

	Consumption
	≤3W

	working temperature
	-20℃~ +70℃

	Infrared wavelength
	850nm

	Infrared lamp quantity
	Φ5 12LED light

	Infrared lamp Irradiation distance
	5M

	Infrared lamp turn on brightness
	＞3Lux

	Connector
	VIDEO OUT (Appropriative aviation connector)

	Size
	Φ68.8mm*59.2mm
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