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Product Parameters
The M16Hv series uses a mini body, which can be easily installed and used in small spaces. Support dual SD card, effectively improve the storage space. The products are compatible with mainstream H.265 video decoding technology, 4G network technology, GPS/BD positioning technology, WIFI technology, etc., which are suitable for all kinds of road patrol vehicles, mixing trucks, logistics vehicles, dump trucks and other industrial vehicles.



Product advantages
· The on-board interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 is optional
· Support 4G, GPS, WIFI function modules
· Rich peripheral interfaces
· Support UI human-computer interface
· Support dual SD card storage
· Support remote system maintenance






Core parameters
	project
	Parameter Description

	Audio and video input
	AHD Video Input
	External 4 * 1080P

	
	Video Standards
	30FPS

	
	Audio Input
	3

	Audio and video output
	CVBS output
	1

	
	VGA output
	1(optional)

	
	Audio Output
	1

	Audio and video parameter encoding
	Video Encoding
	H.264/H.265

	
	Video resolution
	1080P/720P/D1

	
	Audio Coding
	G.711A

	Storage Space
	SD Card
	2, maximum 1TB*2

	Wireless network
	4G Wireless
	1 SIM card​

	
	WIFI
	2.4 / 5.8G ( optional)

	Positioning method
	BeiDou /GPS
	Support, mixed positioning possible

	Interface
	RS232
	1 group

	
	RS485
	1 group

	
	SENSOR
	4

	
	[bookmark: _GoBack]SENSOR OUT
	1

	
	ADC
	2

	
	USB
	1

	
	NET
	1

	Physical specifications
	Size
	135.5mm ( L ) *137.7mm ( W ) *36.5mm ( H )

	
	Weight
	NW：0.5kg，GW：0.75kg
( with a fluctuation of 5% )

	Work Environment
	Operating temperature
	-20 ～ +70 ℃

	
	Operating humidity
	8% ~ 90% (no condensation)

	Other
	Operation Mode
	Remote control, APP , WEB

	
	G SENSOR
	Support
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