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Product introduction
M20Ev series is an integrated design with front and rear dual cameras, 4G, GPS and WIFI. While the rear camera can record the car, the front camera can also record the road information, which has obvious advantages in convenience and security. M20Ev series support H.265 video decoding technology, GPS/BD positioning technology and other mainstream video/network technology.


Product Advantage
· The on-board interface can operate reliably and stably in complex environments
· Video encoding H.265, H.264 is optional
· Support 4G, WIFI, GPS function module
· Supports 2 TF cards. Comes with dual cameras
· Adhesive backing allows for quick installation













Core parameter
	Project
	Parameter Description

	Audio and video input
	Video Input
	Built-in: 2*1080P
External: 2*1080P AHD

	
	Built-in camera perspective
	Outside view：D:130°H:105°V:53°
Inside view：D:157°H:127°V:65°

	
	Video Standards
	25FPS

	
	Audio Input
	1 built-in channel

	Audio and video output
	CVBS output
	Resolution D1, 2-split view
(2 external cameras with 4 partitions)

	
	Audio Output
	built-in

	Audio and video parameter encoding
	Video Encoding
	H.265/H.264

	
	Video resolution
	1080P/720P/D1

	
	Audio Coding
	G.711A

	Storage Space
	TF card
	2, maximum 1TB*2

	Wireless network
	4G Wireless
	1 SIM card

	
	WIFI
	2.4G

	Positioning method
	BeiDou/GPS
	Support, mixed positioning possible

	interface
	RS232
	1 group

	
	SENSOR
	1

	
	SENSOR OUT
	1

	
	ADC
	1

	Physical specifications
	Size
	126 mm (L) * 81.5 mm (W) * 41 mm (H)

	
	Weight
	[bookmark: _GoBack]NW: 0.3 kg GW: 0.65 kg
（with a fluctuation of 5% )

	Work Environment
	Operating temperature
	-20～+70℃

	
	Operating humidity
	8%～90% (no condensation)

	Other
	SOS button
	Support

	
	Collision Sensor
	Support

	
	GSensor
	Support

	
	Linkage alarm
	Acceleration, rollover, collision trigger
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